Government of the People’s Republic of Bangladesh

Office of the Superintending Engineer

Rangpur PWD Circle, Rangpur

Phone: 0521-62512,

Fax: 0521-62422

www.pwd.gov.bd

Memo No: 25.36.8500.110.14.131.16. 2018-**প্রাঃ**  Date: 09.10.16

2nd CORRIGENDUM NOTICE

 This is to inform for all concerned that the following correction have been made in the "Invitation for Tenders" by this office Memo No. 25.36.8500.110.14.001.16.1958-pra Date: 05/09/2016. IFT No. 04 (Civil)/ 2016-2017 Date: 05/09/2016 for " Construction of Chief Judicial Magistrate Court Building of 64 District Head Quarter in Bangladesh. (1st Phase) 1 (One) at Kurigram. (Sub-head : Vertical Extension of Chief Judicial Magistrate Court building from 4th Floor to 7th Floor including Civil, Sanitary & Electrification work ) During the year 2016-2017."

|  |  |  |
| --- | --- | --- |
| BOQ Item NoPart-B Civil Work | As mentioned in Description of Item  | To be replaced by the following Description |
| 1 | 2 | 3 |
| Item No- 44 | Supplying, fitting and fixing 12 mm thick Burma Teak (BT) Veneered board in walling with best quality and well seasoned Garjan wood frame of section 75 x 38 mm at 600 x 600 mm in grid, fitted and fixed to wall by plugs, nails, screws etc. including treatment of inner surface with termite and damp proofing agent maintaining leveled and finished exposed faces including. making holes in wall and mending good the damages. If any, during execution of the work including. cost and carriage of all materials, electricity, accessories, labour for installation, scaffolding, screws, nails etc. including French polishing 3 coats over a coat of priming as per item No. 137 of the schedule etc. all complete as per design, approved sample and accepted by the Engineer. | Supplying, fitting and fixing **plain particle board complying unit wt 499 to 550kg/m**3 , bending strength 0.35N/mm2 , max swelling 8% **, moisture content not more than 10% , for ceiling** of 12 mm thick with best quality and well seasoned Garjan wood frame of section 75 x 38 mm at 600 x 600 mm in grid suspended from **ceiling or roof** or beam by 12 SWG double ply G.I. wire fixed to the ceiling by rowel plug, screws, hooks, nails etc. maintaining straight lines and desired finished level at bottom face with vertical strut as required including cutting holes in slabs or beams by electric drill machine and mending good the damages, if any, during execution of the work including cost and carriage of all materials, accessories, labour for installation, electricity charge, scaffolding, screws, nails etc. including. painting 2 coats over a coat of priming with best quality and approved colour synthetic enamel as per item no 16.6 of this schedule of etc. all complete as per drawing design and accepted by the Engineer. (All sizes of wood are finished) |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| BOQ Part-C (Sanitary Works) & Part- D (Internal Electrification) | As mentioned in BOQ Quantity | Unit | To be replaced by the following Quantity | To be replaced by the following Unit |
| Part-C- Item No- 31 | 478.51 | Rft | 145.84 | rm |
| Part-D-Item No- 19 | Nill | Nill | 60 | Nos |
| Item No- 20 (i) | 60 | Nos | 83 | Nos |
| Item No- 20 (ii) | 83 | Nos | 100 | Nos |
| Item No- 20 (iii) | 100 | Nos | 75 | Nos |
| Item No- 21 | Set | 01 | 01 | Set |

 All other terms and condition will remain unchanged. This corrigendum will be a part and parcel of this Tender.

(Md. Aminul Islam Khan)

Superintending Engineer,

Rangpur PWD Circle, Rangpur